## Test Case 2.7

Validated Requirements

190: Provide EMU Id information (Functional Requirement)

Description

This test case is verify that given EMU ID is available to TCCU.

Categories

|  |  |
| --- | --- |
| Formal Test | Yes |
| Execution Environment | Lab |
| V-Level | System |
| Function Group | Passenger Information and Entertainment Systems |
| Regression | No |
| Automated | No |
| Single Unit Operation Applicability | Yes |
| Multiple Unit Operation Applicability | No |

Pre-Condition

Set Train in TS4 State for DT-1 Cab

Test Case Design

|  |  |  |
| --- | --- | --- |
| **Nos** | **Action** | **Expected Result** |
| 1 |  | Verify that EMU ID is set to UIC000000000001 in RS configuration. |
| 2 |  | Verify that EMUID of Cab1 sent to TCCU1 is 1. |
| 3 |  | Verify that EMUID of Cab2 sent to TCCU1 is 1 |
| 4 | Deactivate DT-1 cab and activate DT-2 cab | |
| 5 |  | Verify that EMUID of Cab1 sent to TCCU2 is 1. |
| 6 |  | Verify that EMUID of Cab2 sent to TCCU2 is 1. |
| 7 | Deactivate DT-2 cab | |

Post-Condition

Set Train State is TS1.